Par Statistics
Total Non-vccgnd Signals=320
Total Non-vccgnd Design Pins=1144
Total Non-vccgnd Conns=1144
Total Non-vccgnd Timing Constrained Conns=672
Phase 1 CPU=3.9 sec
Phase 2 CPU=4.0 sec
Phase 3 CPU=4.8 sec
Phase 4 CPU=5.2 sec
Phase 5 CPU=5.6 sec
Phase 6 CPU=5.6 sec
Phase 7 CPU=5.6 sec
Phase 8 CPU=5.6 sec
Phase 9 CPU=5.6 sec
Phase 10 CPU=5.7 sec
AvgWirelenPerPin Fanout 1=10.0
AvgWirelenPerPin Fanout 2=5.5
AvgWirelenPerPin Fanout 3=9.7
AvgWirelenPerPin Fanout 4=3.8
AvgWirelenPerPin Fanout 10=4.6
AvgWirelenPerPin Fanout 50=6.0
AvgWirelenPerPin Fanout 100=11.0
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.1655