Par Statistics
Total Non-vccgnd Signals=7649
Total Non-vccgnd Design Pins=29439
Total Non-vccgnd Conns=29439
Total Non-vccgnd Timing Constrained Conns=28400
Phase 1 CPU=7.3 sec
Phase 2 CPU=8.0 sec
Phase 3 CPU=22.4 sec
Phase 4 CPU=23.0 sec
Phase 5 CPU=53.5 sec
Phase 6 CPU=53.5 sec
Phase 7 CPU=53.5 sec
Phase 8 CPU=53.5 sec
Phase 9 CPU=54.0 sec
Phase 10 CPU=55.9 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=4.0
AvgWirelenPerPin Fanout 3=4.3
AvgWirelenPerPin Fanout 4=7.0
AvgWirelenPerPin Fanout 10=5.5
AvgWirelenPerPin Fanout 50=4.5
AvgWirelenPerPin Fanout 100=7.8
AvgWirelenPerPin Fanout 500=3.9
AvgWirelenPerPin Fanout 5000=4.5
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=72.1749