Par Statistics
Total Non-vccgnd Signals=7649
Total Non-vccgnd Design Pins=29448
Total Non-vccgnd Conns=29448
Total Non-vccgnd Timing Constrained Conns=28417
Phase 1 CPU=6.7 sec
Phase 2 CPU=7.4 sec
Phase 3 CPU=23.2 sec
Phase 4 CPU=24.9 sec
Phase 5 CPU=127.6 sec
Phase 6 CPU=127.6 sec
Phase 7 CPU=127.6 sec
Phase 8 CPU=127.6 sec
Phase 9 CPU=128.0 sec
Phase 10 CPU=129.8 sec
AvgWirelenPerPin Fanout 1=5.0
AvgWirelenPerPin Fanout 2=4.5
AvgWirelenPerPin Fanout 3=5.0
AvgWirelenPerPin Fanout 4=6.5
AvgWirelenPerPin Fanout 10=5.2
AvgWirelenPerPin Fanout 50=5.1
AvgWirelenPerPin Fanout 100=9.0
AvgWirelenPerPin Fanout 500=4.1
AvgWirelenPerPin Fanout 5000=5.4
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=86.4627