Par Statistics
Total Non-vccgnd Signals=7494
Total Non-vccgnd Design Pins=27012
Total Non-vccgnd Conns=27012
Total Non-vccgnd Timing Constrained Conns=25960
Phase 1 CPU=5.7 sec
Phase 2 CPU=6.4 sec
Phase 3 CPU=21.0 sec
Phase 4 CPU=21.6 sec
Phase 5 CPU=55.5 sec
Phase 6 CPU=55.5 sec
Phase 7 CPU=55.5 sec
Phase 8 CPU=55.5 sec
Phase 9 CPU=55.9 sec
Phase 10 CPU=57.6 sec
AvgWirelenPerPin Fanout 1=5.0
AvgWirelenPerPin Fanout 2=4.5
AvgWirelenPerPin Fanout 3=5.0
AvgWirelenPerPin Fanout 4=6.3
AvgWirelenPerPin Fanout 10=5.8
AvgWirelenPerPin Fanout 50=4.9
AvgWirelenPerPin Fanout 100=9.8
AvgWirelenPerPin Fanout 500=9.0
AvgWirelenPerPin Fanout 5000=6.7
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=69.0417